- General
  TEC1
  TEC ON
  Temperature Sensor
  Temperature Reading: 25.2 ℃
  Temperature Control (℃)
  Set Value
  OFF ON

  TEC2
  TEC ON
  Temperature Sensor
  Temperature Reading: 25.2 ℃
  Temperature Control (℃)
  Set Value
  OFF ON

  TEC3
  TEC ON
  Temperature Sensor
  Temperature Reading: 25.2 ℃
  Temperature Control (℃)
  Set Value
  OFF ON

- Optical Frequency Comb
  Set Central Wavelength (nm)
  Set Value
  OFF ON

  Set Comb Frequency Spacing (GHz)
  Set Value
  OFF ON

  - Master Laser
    - Variable Optical Attenuator - ID: VOA 1
      Current Control (mA)
      Current Reading : mA
      Set Value
      OFF ON

    - Slave Laser
      - Section 1 - ID: Slave 1
        Current Control (mA)
        Current Reading : mA
        Set Value
        OFF ON

  - Comb Tap Output
    - Variable Optical Attenuator - ID: VOA 2
      Current Control (mA)
      Current Reading : mA
      Set Value
      OFF ON

    - Slave Laser
      - Section 1 - ID: Slave 2
        Current Control (mA)
        Current Reading : mA
        Set Value
        OFF ON

- 4 Channel Demultiplexer
  Set Demultiplexer Output 1
  Set Output Power (dBm)
  OFF ON

  Set Demultiplexer Output 2
  Set Output Power (dBm)
  OFF ON

  Set Demultiplexer Output 3
  Set Output Power (dBm)
  OFF ON

  Set Demultiplexer Output 4
  Set Output Power (dBm)
  OFF ON

  - 1:4 Coupler
    Current Control (mA)
    Current Reading : mA
    Set Value
    OFF ON

  - Demultiplexer 1
    - Section 1 - ID: Demux1 Reflector
      Current Control (mA)
      Current Reading : mA
      Set Value
      OFF ON

    - Section 2 - ID Demux1 Gain
      Current Control (mA)
      Current Reading : mA
      Set Value
      OFF ON

  - Demultiplexer 2
    - Section 1 - ID: Demux1 Reflector
      Current Control (mA)
      Current Reading : mA
      Set Value
      OFF ON

    - Section 2 - ID Demux1 Gain
      Current Control (mA)
      Current Reading : mA
      Set Value
      OFF ON

  - Demultiplexer 3
    - Section 1 - ID: Demux1 Reflector
      Current Control (mA)
      Current Reading : mA
      Set Value
      OFF ON

    - Section 2 - ID Demux1 Gain
      Current Control (mA)
      Current Reading : mA
      Set Value
      OFF ON

  - Demultiplexer 4
    - Section 1 - ID: Demux1 Reflector
      Current Control (mA)
      Current Reading : mA
      Set Value
      OFF ON

    - Section 2 - ID Demux1 Gain
      Current Control (mA)
      Current Reading : mA
      Set Value
      OFF ON

×
- Administration
- Status
- SetUp
- Support

#### Set Up Email

Recipient email
Sender email
Authentication (Y/N)
Password
SMTP Server
Port Number
Alert messages ON
Info
Warning
Alert

#### Modal Header

Some text in the modal.

This action requires confirmation

Please enter password

Wrong Password !

###### Please turn off the central wavelength state

#### Idrives are in protected mode