- General
  TEC1
  TEC ON
  Temperature Sensor
  Temperature Reading: 25.2 ℃
  Temperature Control (℃)
  Set Value
  OFF ON

  TEC2
  TEC ON
  Temperature Sensor
  Temperature Reading: 25.2 ℃
  Temperature Control (℃)
  Set Value
  OFF ON

- Tunable Laser
  Laser1
  Set Central Wavelength (nm)
  Set Value
  OFF ON

  Power (dbm)
  Set Value
  OFF ON

  Laser2
  Set Central Wavelength (nm)
  Set Value
  OFF ON

  Power (dbm)
  Set Value
  OFF ON

- Sweep Mode
  Sweep1
  Start Wavelength (nm)
  Stop Wavelength (nm)
  Wavelength Incre. Step (nm)
  Rep. Rate (sweeps/sec)
  Chirp BW (GHz)
  Chirp Freq. (kHz)
  Sweep2
  Start Wavelength (nm)
  Stop Wavelength (nm)
  Wavelength Incre. Step (nm)
  Rep. Rate (sweeps/sec)
  Chirp BW (GHz)
  Chirp Freq. (kHz)

×
- Administration
- Status
- SetUp
- Support

#### Set Up Email

Recipient email
Sender email
Authentication (Y/N)
Password
SMTP Server
Port Number
Alert messages ON
Info
Warning
Alert

#### Modal Header

Some text in the modal.

This action requires confirmation

Please enter password

Wrong Password !

###### Please turn off the central wavelength state

#### Idrives are in protected mode